Current configuration : 12348 bytes
!
! Last configuration change at 14:50:05 UTC Tue Oct 24 2023 by admin
!
version 16.12
no service pad
service timestamps debug datetime msec
service timestamps log datetime msec
service call-home
no platform punt-keepalive disable-kernel-core
!
hostname 1st_Plt_Switch
!
!
vrf definition Mgmt-vrf
 !
 address-family ipv4
 exit-address-family
 !
 address-family ipv6
 exit-address-family
!
enable secret 9 $9$OskBuLWP800Gu.$pbu8Tqf8.X8HY/Yg3pN1AtrRu2TWk6vQArlKSlRnDfI
!
aaa new-model
!
!
!
!
!
!
!
!
aaa session-id common
switch 1 provision ws-c3850-24t
!
!
!
!
call-home
 ! If contact email address in call-home is configured as sch-smart-licensing@cisco.com
 ! the email address configured in Cisco Smart License Portal will be used as contact email address to send SCH notifications.
 contact-email-addr sch-smart-licensing@cisco.com
 profile "CiscoTAC-1"
  active
  destination transport-method http
  no destination transport-method email
ip routing
!
!
!
!
!
ip domain name 1stplt.dco.mil
!
ip dhcp pool DHCP
 network 10.1.10.0 255.255.255.128
 default-router 10.1.10.1
 dns-server 10.1.10.162 10.1.10.163
!
!
!
login on-success log
!
!
!
!
!
!
!
vtp domain dco.mil
vtp mode off
no device-tracking logging theft
!
crypto pki trustpoint SLA-TrustPoint
 revocation-check crl
!
crypto pki trustpoint TP-self-signed-3800366437
 enrollment selfsigned
 subject-name cn=IOS-Self-Signed-Certificate-3800366437
 revocation-check none
 rsakeypair TP-self-signed-3800366437
!
crypto pki trustpoint TP-self-signed-3384119059
 enrollment selfsigned
 subject-name cn=IOS-Self-Signed-Certificate-3384119059
 revocation-check none
 rsakeypair TP-self-signed-3384119059
!
!
crypto pki certificate chain SLA-TrustPoint
 certificate ca 01
  30820321 30820209 A0030201 02020101 300D0609 2A864886 F70D0101 0B050030
  32310E30 0C060355 040A1305 43697363 6F312030 1E060355 04031317 43697363
  6F204C69 63656E73 696E6720 526F6F74 20434130 1E170D31 33303533 30313934
  3834375A 170D3338 30353330 31393438 34375A30 32310E30 0C060355 040A1305
  43697363 6F312030 1E060355 04031317 43697363 6F204C69 63656E73 696E6720
  526F6F74 20434130 82012230 0D06092A 864886F7 0D010101 05000382 010F0030
  82010A02 82010100 A6BCBD96 131E05F7 145EA72C 2CD686E6 17222EA1 F1EFF64D
  CBB4C798 212AA147 C655D8D7 9471380D 8711441E 1AAF071A 9CAE6388 8A38E520
  1C394D78 462EF239 C659F715 B98C0A59 5BBB5CBD 0CFEBEA3 700A8BF7 D8F256EE
  4AA4E80D DB6FD1C9 60B1FD18 FFC69C96 6FA68957 A2617DE7 104FDC5F EA2956AC
  7390A3EB 2B5436AD C847A2C5 DAB553EB 69A9A535 58E9F3E3 C0BD23CF 58BD7188
  68E69491 20F320E7 948E71D7 AE3BCC84 F10684C7 4BC8E00F 539BA42B 42C68BB7
  C7479096 B4CB2D62 EA2F505D C7B062A4 6811D95B E8250FC4 5D5D5FB8 8F27D191
  C55F0D76 61F9A4CD 3D992327 A8BB03BD 4E6D7069 7CBADF8B DF5F4368 95135E44
  DFC7C6CF 04DD7FD1 02030100 01A34230 40300E06 03551D0F 0101FF04 04030201
  06300F06 03551D13 0101FF04 05300301 01FF301D 0603551D 0E041604 1449DC85
  4B3D31E5 1B3E6A17 606AF333 3D3B4C73 E8300D06 092A8648 86F70D01 010B0500
  03820101 00507F24 D3932A66 86025D9F E838AE5C 6D4DF6B0 49631C78 240DA905
  604EDCDE FF4FED2B 77FC460E CD636FDB DD44681E 3A5673AB 9093D3B1 6C9E3D8B
  D98987BF E40CBD9E 1AECA0C2 2189BB5C 8FA85686 CD98B646 5575B146 8DFC66A8
  467A3DF4 4D565700 6ADF0F0D CF835015 3C04FF7C 21E878AC 11BA9CD2 55A9232C
  7CA7B7E6 C1AF74F6 152E99B7 B1FCF9BB E973DE7F 5BDDEB86 C71E3B49 1765308B
  5FB0DA06 B92AFE7F 494E8A9E 07B85737 F3A58BE1 1A48A229 C37C1E69 39F08678
  80DDCD16 D6BACECA EEBC7CF9 8428787B 35202CDC 60E4616A B623CDBD 230E3AFB
  418616A9 4093E049 4D10AB75 27E86F73 932E35B5 8862FDAE 0275156F 719BB2F0
  D697DF7F 28
        quit
crypto pki certificate chain TP-self-signed-3800366437
 certificate self-signed 01
  30820330 30820218 A0030201 02020101 300D0609 2A864886 F70D0101 05050030
  31312F30 2D060355 04031326 494F532D 53656C66 2D536967 6E65642D 43657274
  69666963 6174652D 33383030 33363634 3337301E 170D3233 30343035 31333435
  31355A17 0D333030 31303130 30303030 305A3031 312F302D 06035504 03132649
  4F532D53 656C662D 5369676E 65642D43 65727469 66696361 74652D33 38303033
  36363433 37308201 22300D06 092A8648 86F70D01 01010500 0382010F 00308201
  0A028201 0100AD8A B999EB92 AD5AB864 BF6C2079 0EF9B546 3040FBCD BE781ADD
  77EEC990 E8CB1FB8 EB971471 AEED7B6B 4951005E 0289667A DDB74E13 917403FE
  E30A5257 DAEF32C1 A90E2C82 B04814EC 10803963 E7033BD9 A05E09EB 1DD86788
  8B528560 6E3761A7 6D92D2A5 A11E72B8 3D132D37 97BDD2B6 F7E1F67D C3208B33
  1744083D 759D1400 0198E81B 7F01C53A C7F81DAF 93629DB0 9E423D6A DF76E61C
  1C1DADD6 181ABA20 D86796C8 A68C91C5 8B49CF73 36CC33FB 847F30BC 61B46590
  57476ECD 3CFB6CEE 5FB54424 C9DD7F89 4080B9C7 CD70E6DE 4A47D8C7 FBE04A92
  CAED8597 07361B0E 2A76BED6 71D155BA 913024B1 245BC040 CAC337B8 849711B7
  BCA66AC8 54A70203 010001A3 53305130 0F060355 1D130101 FF040530 030101FF
  301F0603 551D2304 18301680 1413F83D 504DAAB1 D9927A4F 04E4D696 EB7BAFAB
  39301D06 03551D0E 04160414 13F83D50 4DAAB1D9 927A4F04 E4D696EB 7BAFAB39
  300D0609 2A864886 F70D0101 05050003 82010100 45BC1C1A F68F49C1 2C2BDCED
  80ED19BA C8606730 DA5712EB C6EF7BE3 D9AD37C9 5B9EA63A E17F3115 CCA45C14
  75C34FF9 B781472A DDB10304 844E31B8 1F1E4C69 924FF820 53BE9DDB 47596F1E
  08014652 9AE1749A 976F9CB4 D9E02AA7 F1737462 A0323DD9 105D5C0A 562065CF
  59BEE816 50F2142C 96FB4BD1 7E2DF67B 2F795A49 22972B09 E1F0099C 08D8312B
  BE5C94DB 3BE08A33 247EDB30 8FB1F5AE 4C5BB4B7 B5551B2E D59CBA3B 956E11FF
  7B52EF84 DF75B054 027B187B D1EBC07A BE3610D2 7F89B3F0 68CAB1DB 72C1C864
  81FE6FED 249C854E 92A8C461 C12A1F75 9030C624 9F5BE259 36ADCF9F CBC88B76
  5A223D26 8315EE42 F9ECF366 58F93761 E29C03FC
        quit
crypto pki certificate chain TP-self-signed-3384119059
!
!
license boot level ipservicesk9
!
!
diagnostic bootup level minimal
!
spanning-tree mode rapid-pvst
spanning-tree extend system-id
memory free low-watermark processor 79468
!
username admin password 0 DM55Password!@
!
redundancy
 mode sso
!
!
!
!
!
transceiver type all
 monitoring
!
vlan 3,5
!
vlan 6
 name VMOTION
!
vlan 7
 name Provisioning
!
vlan 10
 name users
!
vlan 40
 name DMZ
!
vlan 60
!
!
class-map match-any system-cpp-police-topology-control
  description Topology control
class-map match-any system-cpp-police-sw-forward
  description Sw forwarding, L2 LVX data, LOGGING
class-map match-any system-cpp-default
  description EWLC control, EWLC data, Inter FED
class-map match-any system-cpp-police-sys-data
  description Learning cache ovfl, High Rate App, Exception, EGR Exception, NFL SAMPLED DATA, RPF Failed
class-map match-any system-cpp-police-punt-webauth
  description Punt Webauth
class-map match-any system-cpp-police-l2lvx-control
  description L2 LVX control packets
class-map match-any system-cpp-police-forus
  description Forus Address resolution and Forus traffic
class-map match-any system-cpp-police-multicast-end-station
  description MCAST END STATION
class-map match-any system-cpp-police-multicast
  description Transit Traffic and MCAST Data
class-map match-any system-cpp-police-l2-control
  description L2 control
class-map match-any system-cpp-police-dot1x-auth
  description DOT1X Auth
class-map match-any system-cpp-police-data
  description ICMP redirect, ICMP_GEN and BROADCAST
class-map match-any system-cpp-police-stackwise-virt-control
  description Stackwise Virtual
class-map match-any non-client-nrt-class
class-map match-any system-cpp-police-routing-control
  description Routing control and Low Latency
class-map match-any system-cpp-police-protocol-snooping
  description Protocol snooping
class-map match-any system-cpp-police-dhcp-snooping
  description DHCP snooping
class-map match-any system-cpp-police-system-critical
  description System Critical and Gold Pkt
!
policy-map system-cpp-policy
!
!
!
!
!
!
!
!
!
!
!
interface Port-channel1
 switchport trunk allowed vlan 10,20,30
 switchport mode trunk
!
interface GigabitEthernet0/0
 vrf forwarding Mgmt-vrf
 no ip address
 shutdown
 negotiation auto
!
interface GigabitEthernet1/0/1
 description Cyber Pack VSWI
 switchport trunk native vlan 100
 switchport trunk allowed vlan 3,10,20,30,40,50
 switchport mode trunk
 switchport nonegotiate
 spanning-tree portfast trunk
!
interface GigabitEthernet1/0/2
 description MiniRax1 VSWI
 switchport trunk allowed vlan 10,20,30
 switchport mode trunk
!
interface GigabitEthernet1/0/3
 description MiniRax2 VSWI
 switchport trunk allowed vlan 10,30
 switchport mode trunk
!
interface GigabitEthernet1/0/4
 description MiniRax3 VSWI
 switchport trunk allowed vlan 10,30
 switchport mode trunk
!
interface GigabitEthernet1/0/5
 description CyberPax MGMT
 switchport trunk native vlan 100
 switchport trunk allowed vlan 5-8
 switchport mode trunk
 switchport nonegotiate
 spanning-tree portfast trunk
!
interface GigabitEthernet1/0/6
 description MiniRax1 MGMT
 switchport trunk native vlan 100
 switchport trunk allowed vlan 5-8
 switchport mode trunk
!
interface GigabitEthernet1/0/7
 description MiniRax2 MGMT
 switchport trunk native vlan 100
 switchport trunk allowed vlan 5-8
 switchport mode trunk
!
interface GigabitEthernet1/0/8
 description MiniRax3 MGMT
 switchport trunk native vlan 100
 switchport trunk allowed vlan 5-8
 switchport mode trunk
!
interface GigabitEthernet1/0/9
 description Gigamon MGMT
 switchport access vlan 10
 switchport mode access
!
interface GigabitEthernet1/0/10
 description NAS MGMT
 switchport access vlan 10
 switchport mode access
!
interface GigabitEthernet1/0/11
 description NAS Link
 switchport access vlan 20
 switchport mode access
!
interface GigabitEthernet1/0/12
 description IPMI
 switchport access vlan 10
 switchport mode access
!
interface GigabitEthernet1/0/13
 description Laptop
 switchport access vlan 5
!
interface GigabitEthernet1/0/14
 description Laptop
 switchport access vlan 60
 switchport mode access
!
interface GigabitEthernet1/0/15
 description Laptop
 switchport access vlan 60
!
interface GigabitEthernet1/0/16
 description Laptop
 switchport access vlan 60
!
interface GigabitEthernet1/0/17
 description Laptop
 switchport access vlan 60
!
interface GigabitEthernet1/0/18
 description Laptop
 switchport access vlan 60
!
interface GigabitEthernet1/0/19
 description Laptop
 switchport access vlan 60
!
interface GigabitEthernet1/0/20
 description Laptop
 switchport access vlan 60
!
interface GigabitEthernet1/0/21
 description Laptop
 switchport access vlan 60
!
interface GigabitEthernet1/0/22
 description Laptop
 switchport access vlan 60
!
interface GigabitEthernet1/0/23
 description Laptop
 switchport access vlan 60
!
interface GigabitEthernet1/0/24
 description Laptop
 switchport access vlan 3
!
interface GigabitEthernet1/1/1
!
interface GigabitEthernet1/1/2
!
interface GigabitEthernet1/1/3
!
interface GigabitEthernet1/1/4
!
interface TenGigabitEthernet1/1/1
!
interface TenGigabitEthernet1/1/2
!
interface TenGigabitEthernet1/1/3
!
interface TenGigabitEthernet1/1/4
!
interface Vlan1
 no ip address
 shutdown
!
interface Vlan3
 description Routing Interface
 ip address 10.1.3.1 255.255.255.0
!
interface Vlan5
 description ESXi Management
 ip address 10.1.5.1 255.255.255.0
!
interface Vlan6
 description ESXi vMotion
 ip address 10.1.6.1 255.255.255.0
!
interface Vlan7
 description ESXi Provisioning
 ip address 10.1.7.1 255.255.255.0
!
interface Vlan10
 description Domain Services
 ip address 10.1.10.1 255.255.255.0
!
interface Vlan20
 description ***MANAGEMENT***
 no ip address
!
interface Vlan30
 description ***SERVERS***
 no ip address
!
interface Vlan40
 description Host Data Collection
 no ip address
!
interface Vlan60
 description USER
 ip address 10.1.60.1 255.255.255.0
!
ip forward-protocol nd
ip http server
ip http authentication local
ip http secure-server
ip route 0.0.0.0 0.0.0.0 10.1.3.2
ip route 10.0.0.0 255.255.0.0 10.0.3.1
ip route 10.1.15.0 255.255.255.0 10.0.3.4
ip route 10.1.16.0 255.255.255.0 10.0.3.4
ip route 10.1.20.0 255.255.255.0 10.0.3.4
ip route 10.1.30.0 255.255.255.0 10.0.3.4
ip route 10.1.40.0 255.255.255.0 10.0.3.14
ip route 10.1.50.0 255.255.255.0 10.0.3.4
ip route 10.2.0.0 255.255.0.0 10.0.3.5
ip route 10.3.0.0 255.255.0.0 10.0.3.7
!
!
!
!
!
!
!
!
control-plane
 service-policy input system-cpp-policy
!
!
line con 0
 logging synchronous
 stopbits 1
line aux 0
 stopbits 1
line vty 0 4
 transport input ssh
line vty 5 15
 transport input ssh
!
!
!
!
!
!
!
end