fileshare: \\10.1.10.14 Administrator standard
ESXi – 10.1.5.11 root standard
IPMI-10.1.5.12 admin standard
SecOnion -- 10.1.10.22 soadmin@3rdplt.dco.mil
PaloAlto -- 10.1.10.21 admin
DC1 -- 10.1.10.14
DC2 -- 10.1.10.15
Splunk_ID1 -- 10.1.10.25:8000   administrator standard
Splunk_ID2 -- 10.1.10.26:8000 
Splunk_SH -- 10.1.10.24:8000
Arkime – 10.1.10.80 amin standard no !@

Virtual Networking
Virtual switches 
	Domain Services
		VMNIC-2
	Firewall External
		VMNIC-	4
	Sniffing
		VMNIC-3
	Vswitch0
		VMNIC-0 Management
		VMNIC-1 IPMI

Port groups
	Domain Services vlan id 0
	Firewall External vlan id 0
	Sniffing vlan id 4095
	VM Network vlan id 0
	Management network vlan id 4095 

SWITCH CONFIGURATION

Current configuration : 10454 bytes
!
! Last configuration change at 17:08:16 UTC Wed Feb 28 2024
!
version 16.12
no service pad
service timestamps debug datetime msec
service timestamps log datetime msec
service call-home
platform punt-keepalive disable-kernel-core
!
hostname Switch
!
!
vrf definition Mgmt-vrf
 !
 address-family ipv4
 exit-address-family
 !
 address-family ipv6
 exit-address-family
!
!
no aaa new-model
switch 1 provision ws-c3850-24t
!
!
!
!
call-home
 ! If contact email address in call-home is configured as sch-smart-licensing@cisco.com
 ! the email address configured in Cisco Smart License Portal will be used as contact email address to send SCH notifications.
 contact-email-addr sch-smart-licensing@cisco.com
 profile "CiscoTAC-1"
  active
  destination transport-method http
  no destination transport-method email
ip routing
!
!
!
!
!
!
ip dhcp pool ***USERS***
 network 10.1.10.0 255.255.255.0
 default-router 10.1.10.1
 dns-server 10.1.10.14
!
!
!
login on-success log
!
!
!
!
!
no device-tracking logging theft
!
crypto pki trustpoint SLA-TrustPoint
 enrollment pkcs12
 revocation-check crl
!
crypto pki trustpoint TP-self-signed-2768369970
 enrollment selfsigned
 subject-name cn=IOS-Self-Signed-Certificate-2768369970
 revocation-check none
 rsakeypair TP-self-signed-2768369970
!
!
crypto pki certificate chain SLA-TrustPoint
 certificate ca 01
  30820321 30820209 A0030201 02020101 300D0609 2A864886 F70D0101 0B050030
  32310E30 0C060355 040A1305 43697363 6F312030 1E060355 04031317 43697363
  6F204C69 63656E73 696E6720 526F6F74 20434130 1E170D31 33303533 30313934
  3834375A 170D3338 30353330 31393438 34375A30 32310E30 0C060355 040A1305
  43697363 6F312030 1E060355 04031317 43697363 6F204C69 63656E73 696E6720
  526F6F74 20434130 82012230 0D06092A 864886F7 0D010101 05000382 010F0030
  82010A02 82010100 A6BCBD96 131E05F7 145EA72C 2CD686E6 17222EA1 F1EFF64D
  CBB4C798 212AA147 C655D8D7 9471380D 8711441E 1AAF071A 9CAE6388 8A38E520
  1C394D78 462EF239 C659F715 B98C0A59 5BBB5CBD 0CFEBEA3 700A8BF7 D8F256EE
  4AA4E80D DB6FD1C9 60B1FD18 FFC69C96 6FA68957 A2617DE7 104FDC5F EA2956AC
  7390A3EB 2B5436AD C847A2C5 DAB553EB 69A9A535 58E9F3E3 C0BD23CF 58BD7188
  68E69491 20F320E7 948E71D7 AE3BCC84 F10684C7 4BC8E00F 539BA42B 42C68BB7
  C7479096 B4CB2D62 EA2F505D C7B062A4 6811D95B E8250FC4 5D5D5FB8 8F27D191
  C55F0D76 61F9A4CD 3D992327 A8BB03BD 4E6D7069 7CBADF8B DF5F4368 95135E44
  DFC7C6CF 04DD7FD1 02030100 01A34230 40300E06 03551D0F 0101FF04 04030201
  06300F06 03551D13 0101FF04 05300301 01FF301D 0603551D 0E041604 1449DC85
  4B3D31E5 1B3E6A17 606AF333 3D3B4C73 E8300D06 092A8648 86F70D01 010B0500
  03820101 00507F24 D3932A66 86025D9F E838AE5C 6D4DF6B0 49631C78 240DA905
  604EDCDE FF4FED2B 77FC460E CD636FDB DD44681E 3A5673AB 9093D3B1 6C9E3D8B
  D98987BF E40CBD9E 1AECA0C2 2189BB5C 8FA85686 CD98B646 5575B146 8DFC66A8
  467A3DF4 4D565700 6ADF0F0D CF835015 3C04FF7C 21E878AC 11BA9CD2 55A9232C
  7CA7B7E6 C1AF74F6 152E99B7 B1FCF9BB E973DE7F 5BDDEB86 C71E3B49 1765308B
  5FB0DA06 B92AFE7F 494E8A9E 07B85737 F3A58BE1 1A48A229 C37C1E69 39F08678
  80DDCD16 D6BACECA EEBC7CF9 8428787B 35202CDC 60E4616A B623CDBD 230E3AFB
  418616A9 4093E049 4D10AB75 27E86F73 932E35B5 8862FDAE 0275156F 719BB2F0
  D697DF7F 28
        quit
crypto pki certificate chain TP-self-signed-2768369970
 certificate self-signed 01
  30820330 30820218 A0030201 02020101 300D0609 2A864886 F70D0101 05050030
  31312F30 2D060355 04031326 494F532D 53656C66 2D536967 6E65642D 43657274
  69666963 6174652D 32373638 33363939 3730301E 170D3234 30323136 31353036
  32385A17 0D333030 31303130 30303030 305A3031 312F302D 06035504 03132649
  4F532D53 656C662D 5369676E 65642D43 65727469 66696361 74652D32 37363833
  36393937 30308201 22300D06 092A8648 86F70D01 01010500 0382010F 00308201
  0A028201 0100FEEC B71FD84C ACCA47EC 71C16C4B E51D1780 42E937D0 C232209D
  29330F03 23651329 B47C9841 E192835B 92CE18D6 61E30D29 2ECBCAEC 752441EC
  7E45E18A EB4FF99B EC4165EB 443B1CDC 58293373 B8ACFE3B F8DE8D88 C3573AF2
  CF023FAC FBA73794 AF3E6BC0 997327C7 3C41C854 E5F29ECC 52B57608 8B0C0912
  D0108E1D 27B44EC7 ADE7229A 1B610DB1 98C5F48C 4A81DFBA BAB445CD A54D5E47
  D6CDCCB5 E7C10CC7 163FE42F 16D19C39 00BBFA23 583CB683 F2531B04 32C3C87B
  F325488F 138388D8 04A9983B EBB40705 53585BA7 7DD91159 55481572 CB5D07F6
  7B75BAF0 FD4EC214 179384C0 83FE1F49 1602994E 17639B9B FEA54CB9 AB3B4DF9
  9F5FEB23 51FD0203 010001A3 53305130 0F060355 1D130101 FF040530 030101FF
  301F0603 551D2304 18301680 149FE266 BE413AD2 E9C4EB10 BEC9DB3A 40945BC0
  83301D06 03551D0E 04160414 9FE266BE 413AD2E9 C4EB10BE C9DB3A40 945BC083
  300D0609 2A864886 F70D0101 05050003 82010100 1F16CA8C 4AF5AA95 C5625FAE
  5E127809 97A3D66C 9542A6CA F9AADF74 9D693E13 6A715ABE AB7592BA 95287F3F
  11D3BF91 F0911849 10E5CE14 3BB91606 974549A9 C8504624 1864F51F 46A14F64
  0D434DE7 93AEA8A2 1E5F6690 4F573BC8 FBEF3229 7671D72A 09AE0E94 452845BD
  4EB41F81 F1B3E7A0 D5583E13 55AE98F0 57C6FB7B 96036026 CDFD0584 A7119909
  B5D53276 6AB213B5 D59743A4 7D81CFE1 35C1D9F4 EA4EA7AC 5F096956 8CBFF824
  80D5FECB 7170E24E 43F941A4 084BE9C4 3870FE40 32FF66E8 01C42C07 EAE0BBA9
  AFDA777E 2AC1D9F4 AA0282E7 A5594AEC 408DFD21 EB5FED94 E6159872 A7D9499B
  27105D9D 4388AA63 22F97356 33BE9E7A 2EDC7197
        quit
!
!
!
diagnostic bootup level minimal
!
spanning-tree mode rapid-pvst
spanning-tree extend system-id
memory free low-watermark processor 79475
!
!
redundancy
 mode sso
!
!
!
!
!
transceiver type all
 monitoring
!
!
class-map match-any system-cpp-police-topology-control
  description Topology control
class-map match-any system-cpp-police-sw-forward
  description Sw forwarding, L2 LVX data, LOGGING
class-map match-any system-cpp-default
  description EWLC control, EWLC data, Inter FED
class-map match-any system-cpp-police-sys-data
  description Learning cache ovfl, High Rate App, Exception, EGR Exception, NFL SAMPLED DATA, RPF Failed
class-map match-any system-cpp-police-punt-webauth
  description Punt Webauth
class-map match-any system-cpp-police-l2lvx-control
  description L2 LVX control packets
class-map match-any system-cpp-police-forus
  description Forus Address resolution and Forus traffic
class-map match-any system-cpp-police-multicast-end-station
  description MCAST END STATION
class-map match-any system-cpp-police-multicast
  description Transit Traffic and MCAST Data
class-map match-any system-cpp-police-l2-control
  description L2 control
class-map match-any system-cpp-police-dot1x-auth
  description DOT1X Auth
class-map match-any system-cpp-police-data
  description ICMP redirect, ICMP_GEN and BROADCAST
class-map match-any system-cpp-police-stackwise-virt-control
  description Stackwise Virtual
class-map match-any non-client-nrt-class
class-map match-any system-cpp-police-routing-control
  description Routing control and Low Latency
class-map match-any system-cpp-police-protocol-snooping
  description Protocol snooping
class-map match-any system-cpp-police-dhcp-snooping
  description DHCP snooping
class-map match-any system-cpp-police-system-critical
  description System Critical and Gold Pkt
!
policy-map system-cpp-policy
!
!
!
!
!
!
!
!
!
!
interface GigabitEthernet0/0
 vrf forwarding Mgmt-vrf
 no ip address
 shutdown
 negotiation auto
!
interface GigabitEthernet1/0/1
 description ESXI
 switchport access vlan 20
 switchport mode access
!
interface GigabitEthernet1/0/2
 description ESXI
 switchport access vlan 20
 switchport mode access
!
interface GigabitEthernet1/0/3
 description ESXI
 switchport access vlan 20
 switchport mode access
!
interface GigabitEthernet1/0/4
 description ESXI
 switchport access vlan 20
 switchport mode access
!
interface GigabitEthernet1/0/5
 description ESXI
 switchport access vlan 20
 switchport mode access
!
interface GigabitEthernet1/0/6
 description users
 switchport access vlan 10
 switchport mode access
!
interface GigabitEthernet1/0/7
 description users
 switchport access vlan 10
 switchport mode access
!
interface GigabitEthernet1/0/8
 description users
 switchport access vlan 10
 switchport mode access
!
interface GigabitEthernet1/0/9
 description users
 switchport access vlan 10
 switchport mode access
!
interface GigabitEthernet1/0/10
 description users
 switchport access vlan 10
 switchport mode access
!
interface GigabitEthernet1/0/11
 description users
 switchport access vlan 10
 switchport mode access
!
interface GigabitEthernet1/0/12
 description users
 switchport access vlan 10
 switchport mode access
!
interface GigabitEthernet1/0/13
 description users
 switchport access vlan 10
 switchport mode access
!
interface GigabitEthernet1/0/14
 description users
 switchport access vlan 10
 switchport mode access
!
interface GigabitEthernet1/0/15
 description users
 switchport access vlan 10
 switchport mode access
!
interface GigabitEthernet1/0/16
 description users
 switchport access vlan 10
 switchport mode access
!
interface GigabitEthernet1/0/17
 description users
 switchport access vlan 10
 switchport mode access
!
interface GigabitEthernet1/0/18
 description users
 switchport access vlan 10
 switchport mode access
!
interface GigabitEthernet1/0/19
 description users
 switchport access vlan 10
 switchport mode access
!
interface GigabitEthernet1/0/20
 description users
 switchport access vlan 10
 switchport mode access
!
interface GigabitEthernet1/0/21
 description users
 switchport access vlan 10
 switchport mode access
!
interface GigabitEthernet1/0/22
 description users
 switchport access vlan 10
 switchport mode access
!
interface GigabitEthernet1/0/23
 description users
 switchport access vlan 10
 switchport mode access
!
interface GigabitEthernet1/0/24
 description users
 switchport access vlan 10
 switchport mode access
!
interface GigabitEthernet1/1/1
!
interface GigabitEthernet1/1/2
!
interface GigabitEthernet1/1/3
!
interface GigabitEthernet1/1/4
!
interface TenGigabitEthernet1/1/1
!
interface TenGigabitEthernet1/1/2
!
interface TenGigabitEthernet1/1/3
!
interface TenGigabitEthernet1/1/4
!
interface Vlan1
 no ip address
 shutdown
!
interface Vlan10
 description USERS
 ip address 10.1.10.1 255.255.255.0
!
interface Vlan20
 description ESXI
 ip address 10.1.5.1 255.255.255.0
!
ip forward-protocol nd
ip http server
ip http authentication local
ip http secure-server
!
!
!
!
control-plane
 service-policy input system-cpp-policy
!
!
line con 0
 stopbits 1
line aux 0
 stopbits 1
line vty 0 4
 login
line vty 5 15
 login
!
!
!
!
!
!
!
end